         (0,0)

When calculating pixel coordinates for bin or sum images, the CRO coordinates
include ccd summing and have to be moved back to the coordinate of the lower-left
full resolution pixel before being binned and/or summed.

When making calculations based on the CDL_NCOL/CDL_NLIN values, move back 1 full
binned/summed pixel (which appears to have been included in ’1024’).

                                           MDM V1.0 12-Mar-98; RWN V1.1 24-Feb-00