          (0,0)

On chip summing, means CRO_FPO in full pixel units has to be adjusted by
              1x1 = 0
              2x2 = 0.5 pixels
              4x4 = 1.5 pixels
              8x8 = 3.5 pixels
Shift = (NPIX-1)/2 = (TBIN_CCD - 1)*0.5

Coordinate systems:
  Camera Readout ("CRO") is Summed Pixel Readout
  Full Resolution Solar Rotated Image is "SRI"

                                           MDM V1.0 12-Mar-98; RWN V1.1 24-Feb-00