             (x0,y0)

The center of the image pixel location in units of full-resolution pixels is
x0 + (nx-1)/2 * TBIN_CCD  (= SRI_LLEX + (NX-1)/2. * TBIN_CCD  =  SRI_FOVX)

                                                   MDM V1.0 12-Mar-98; RWN V1.1 24-Feb-00